{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":4,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":41,"n_cols":13,"rows_kept":41,"cut":false,"hidden":false,"merged":[]}
[{"$nulls":5},"旧的",null,"功能选择",null,null,null,"定时器0","系统事件"]
[1,"PWM2/IC6/T0/AIN4/P0.5",null,null,null,"控制",null,"GPIO",null,"按键1",null,"定时器1"]
[2,"TXD/AIN3/P0.6",null,null,null,"调试TX",null,null,"UART0","TX",null,"定时器2"]
[3,"RXD/AIN2/P0.7",null,null,null,"调试RX",null,null,"UART0","RX",null,"定时器3","延时"]
[4,"RST/P2.0",null,null,null,"调试RST"]
[5,"INT0/OSCIN/AIN1/P3.0",null,null,null,"保留ADC1",null,"ADC1",null,"DH11"]
[6,"INT1/AIN0/P1.7",null,null,null,"保留ADC0",null,"ADC0",null,"光敏"]
[7,"GND",null,null,null,"GND"]
[8,"[SDA]/TXD_1/ICPDA/OCDDA/P1.6",null,null,null,"调试DAT",null,null,"UART1","TX_1"]
[9,"VDD",null,null,null,"VDD"]
[10,"PWM5/IC7/SS/P1.5",null,null,null,"SS 片选",null,"SPI",null,"24L01占用"]
[11,"P1.4/SDA/FB/PWM1",null,null,null,"保留I2C_SDA",null,"I2C",null,"霍尔磁性"]
[12,"P1.3/SCL/[STADC]",null,null,null,"保留I2C_SCL",null,"I2C"]
[13,"P1.2/PWM0/IC0",null,null,null,"保留PWM0",null,"PWM0","led","系统LED"]
[14,"P1.1/PWM1/IC1/AIN7/CLO",null,null,null,"SPI_CE",null,"GPIO",null,"24L01占用"]
[15,"P1.0/PWM2/IC2/SPCLK",null,null,null,"SPCLK",null,"SPI",null,"24L01占用"]
[16,"P0.0/PWM3/IC3/MOSI/T1",null,null,null,"MOSI",null,"SPI",null,"24L01占用"]
[17,"P0.1/PWM4/IC4/MISO",null,null,null,"MISO",null,"SPI",null,"24L01占用"]
[18,"P0.2/ICPCK/OCDCK/RXD_1/[SCL]",null,null,null,"调试CLK",null,null,"UART1","RX_1"]
[19,"P0.3/PWM5/IC5/AIN6",null,null,null,"SPI_IRQ中断",null,"中断",null,"24L01占用"]
[20,"P0.4/AIN5/STADC/PWM3/IC3",null,null,null,"控制",null,"GPIO",null,"控制1"]
[]
[null,"24L01",null,"N76E003"]
[null,"GND",null,"GND"]
[null,"VCC",null,"VDD"]
[null,"CE",null,"P1.1",null,null,"使能TX或RX模式"]
[null,"CSN",null,"P1.5",null,null,"片选"]
[null,"SCK",null,"P1.0"]
[null,"MOSI",null,"P0.0"]
[null,"MISO ",null,"P0.1"]
[null,"IRQ",null,"P0.3",null,null,"可屏蔽中断","低有效"]
[]
[]
[]
["功能："]
[1,"2401的spi","中断",null,"**"]
[2,"看门狗",null,null,"*"]
[3,"eeprom掉电保存",null,null,"*"]
[4,"uart打印"]
[5,"gpio控制",null,null,"*"]
[6,"低功耗"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}